PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        15.2.4
   LDD Version Id:        1.1.0.0
   LDD Label Version Id:  1.20
   LDD Discipline (T/F):  false
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Tue Jan 21 15:28:28 UTC 2025
   Common Schema          [PDS4_PDS_1E00.xsd]
   Common Schematron      [PDS4_PDS_1E00.sch]
   IM Version Id:         1.14.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.20
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-lcross/ldd-lcross/src/PDS4_LCROSS_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         false
   Mission LDD            true
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                7
   Attributes             29
   Associations           36
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               LCROSS Mission Dictionary
   LDD Version            1.1.0.0
   Full Name              Jennifer Ward
   Steward                geo
   Namespace Id           lcross
   Comment                
        The LCROSS mission dictionary contains a class with attributes specific to the 
        LCROSS mission and instruments. This dictionary was created for the migration
        of LCROSS data products from PDS3 to PDS4.        
    
   Last Modification Time 2024-11-20
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   product_type
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description             The product_type attributes identifies the type or category of a product within a data set. 

   name                   producer_name
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The name of the person who produced the data product.

   name                   producer_institution_name
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description             The producer_institution_name element identifies a university, research center, NASA center or other institution associated with the production of a data set. 

   name                   mission_phase_name
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description             The mission_phase_name element provides the commonly-used identifier of a mission phase. 

   name                   spacecraft_clock_start_count
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_start_count attribute provides the value of the spacecraft clock at the beginning of a time period of interest. 
   minimum characters     15
   maximum characters     15

   name                   spacecraft_clock_stop_count
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The spacecraft_clock_stop_count attribute provides the value of the spacecraft clock at the end of a time period of interest. 

   name                   intercept_point_latitude
   version                1.14
   value data type        ASCII_Real
   description            The intercept_point_latitude attribute is the latitude of a point on the surface of a body.
   minimum value          -90.0
   maximum value          90.0
   unit of measure type   Units_of_Angle

   name                   intercept_point_longitude
   version                1.14
   value data type        ASCII_Real
   description            The intercept_point_longitude attribute is the longitude of a point on the surface of a body.
   minimum value          0.0
   maximum value          360.0
   unit of measure type   Units_of_Angle

   name                   instrument_temperature
   version                1.14
   value data type        ASCII_Real
   description            The instrument_temperature attribute provides the temperature, in degrees Celsius of an instrument or some part of an instrument.
   unit of measure type   Units_of_Temperature

   name                   instrument_temperature_count
   version                1.14
   value data type        ASCII_Integer
   description            The instrument_temperature_count attribute provides the temperature of an instrument in raw counts or DN values. 

   name                   instrument_gain_state
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The instrument_gain_state specifies the instrument gain state, either High or Low. 

   name                   missing_packet_flag
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The missing_packet_flag indicates whether the image is missing data. A missing packet appears as a horizontal bar 8 pixels high of zero data. 

   name                   calibration_valid
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The response of the mid-IR cameras exhibited a startup transient. The calibration is valid only after this transient had settled. This attribute indicates whether the image was taken before or after this point. Values are Yes or No. 

   name                   enhancement_mode
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            This attribute indicates whether onboard image stretching was enabled or disabled. Values are On or Off. 

   name                   operating_setting_value
   version                1.14
   value data type        ASCII_Integer
   description            The operating setting value determines the integration time and gain. Values range from 0 to 15. 
   minimum value          0
   maximum value          15

   name                   integration_time
   version                1.14
   value data type        ASCII_Integer
   description            The integration time in msec. 
   minimum value          0
   unit of measure type   Units_of_Time

   name                   gain_value
   version                1.14
   value data type        ASCII_Integer
   description            The focal plane sensitivity in electrons per count. Value is approximate and inferred from the operating setting value and factory definitions. 
   minimum value          0

   name                   saturation_flag
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            Indicates whether a spectra is saturated based on a mechanical test. 

   name                   boresight_to_sun_angle
   version                1.14
   value data type        ASCII_Real
   description            Angle between the instrument boresight vector and the spacecraft to sun vector in degrees. 
   unit of measure type   Units_of_Angle

   name                   exposure_duration
   version                1.14
   value data type        ASCII_Real
   description            The time interval between the opening and closing of an instrument aperture. 

   name                   tec_setpoint
   version                1.14
   value data type        ASCII_Real
   description            The setpoint temperature of the VSP thermo-electric cooler. 
   unit of measure type   Units_of_Temperature

   name                   tec_temperature
   version                1.14
   value data type        ASCII_Real
   description            The measurement temperature of the VSP thermo-electric cooler. 
   unit of measure type   Units_of_Temperature

   name                   packet_timestamp
   version                1.14
   value data type        ASCII_Integer
   description            A 32-bit unsigned integer representing time from the epoch Jan 1, 1980 in milliseconds. This counter resets every approximately 50 days. 

   name                   vsp_bracket_number
   version                1.14
   value data type        ASCII_Integer
   description            When in bracket mode, the VSP captures three spectra in quick succession. The bracket number indicates which of the three spectra are captured.. 

   name                   right_ascension_angle
   version                1.14
   value data type        ASCII_Real
   description            The right_ascension_angle attribute provides the value of right ascension (RA) as an angle. Right ascension is measured from the vernal equinox or the first point of Aries, which is the place on the celestial sphere where the Sun crosses the celestial equator from south to north at the March equinox. Right ascension is measured continuously in a full circle from that equinox towards the east. Right ascension is used in conjunction with the declination attribute to specify a point on the sky. 
   unit of measure type   Units_of_Angle

   name                   declination
   version                1.14
   value data type        ASCII_Real
   description            The declination_angle (Dec) attribute provides the value of an angle on the celestial sphere, measured north from the celestial equator to the point in question. (For points south of the celestial equator, negative values are used.) Declination is used in conjunction with right ascension (right_ascension_angle) to specify a point on the sky.
   unit of measure type   Units_of_Angle

   name                   exposure_length
   version                1.14
   value data type        ASCII_Real
   description            Provides the length of time for an exposure.
   unit of measure type   Units_of_Time

   name                   filter_name
   version                1.14
   value data type        ASCII_Short_String_Collapsed
   description            The commonly used name of a filter the is part of an imaging system.

   name                   center_filter_wavelength
   version                1.14
   value data type        ASCII_Real
   description            The center wavelength of a filter used in an imaging system.
   unit of measure type   Units_of_Length

Parsed Input - Classes:

   name                   MIR_Instrument_State
   description            Class with attributes specific to the MIR instrument on LCROSS.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.instrument_gain_state
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.missing_packet_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.calibration_valid
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   NIR_Instrument_State
   description            Class with attributes specific to the NIR instrument on LCROSS.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.enhancement_mode
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.operating_setting_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.integration_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.gain_value
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   NSP_Instrument_State
   description            Class with attributes specific to the NSP instrument on LCROSS.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.saturation_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.boresight_to_sun_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   VSP_Instrument_State
   description            Class with attributes specific to the VSP instrument on LCROSS.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.saturation_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.exposure_duration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.tec_setpoint
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.tec_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.packet_timestamp
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.vsp_bracket_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Ground_Based_Parameters
   description            Container class for ground-based observation parameters.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.right_ascension
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.declination
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.exposure_length
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.filter_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.center_filter_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Mission_Parameters
   description            Container class for mission level attributes (i.e., common across all or most instruments) and instrument specific classes.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.product_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.producer_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.producer_institution_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.mission_phase_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.spacecraft_clock_start_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.spacecraft_clock_stop_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.intercept_point_latitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.intercept_point_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.instrument_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lcross.instrument_temperature_count
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   LCROSS_Parameters
   description            Top level container class.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      lcross.Mission_Parameters
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

      local identifier      lcross.MIR_Instrument_State
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lcross.NIR_Instrument_State
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lcross.NSP_Instrument_State
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lcross.VSP_Instrument_State
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      lcross.Ground_Based_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

End of Report
