PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        14.1.2
   LDD Version Id:        1.11.0.0
   LDD Label Version Id:  1.25
   LDD Discipline (T/F):  true
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Tue Oct 25 22:09:24 UTC 2022
   Common Schema          [PDS4_PDS_1J00.xsd]
   Common Schematron      [PDS4_PDS_1J00.sch]
   IM Version Id:         1.19.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.25
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Configuration File  [MDPTNConfigClassDisp.xml]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-rings/ldd-rings/src/PDS4_RINGS_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         true
   Mission LDD            false
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                21
   Attributes             162
   Associations           296
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               Rings Dictionary
   LDD Version            1.11.0.0
   Full Name              Mitchell K Gordon
   Steward                rings
   Namespace Id           rings
   Comment                 
    
    	Classes used from the geom namespace
    	  - Body_Ident_Base
    	  - Reference_Frame_Ident
    	  - Central_Body_Ident
    	  - Display_Direction
    	  
    	Classes used from the pds namespace
    	  - Internal_Reference

    	Attributes used from the pds namespace
    	  - local_identifier_reference
    	  - sampling_parameter_name
    	  - sampling_parameter_unit
    	  - sampling_parameter_interval
    	  - description
    	  - name     (indirectly via classes from the geom namespace)
    	  - comment  (indirectly via classes from the geom namespace)

      v1.2.0  2014-03-29
        -  Moved information from comments into definitions for all attributes. 
        -  Added source product, orbit number and sclk start/stop times. 
        -  Revised some enumerated value options, and corrected some nillable inconsistencies.
      v1.3.0  2015-01-23
        -  Updated to version 1.3.0.1 of IM.
        -  Added min/max_observed_event_time.
        -  Included reference_time_UTC as optional attribute for all profile labels.
        -  Revised some definitions.
      v1.4.0.0  2016-04-25
        -  This version was not released
        -  Updated to version 1.6.0.0 of IM.
        -  Corrected case errors in class and attribute names and enumerated values
        -  Changed several time attribute types from ASCII_Date_Time_UTC to ASCII_Date_Time_YMD_UTC
        -  revised several definitions
        -  Changed ring_occultation_direction to occultation_direction, and modified the definitions 
           for the values ingress and egress.
        -  Added the class Occultation_Time_Series.
        -  Combined Radio_Occultation and Stellar_Occultation into Occultation_Ring_Profile
        -  Renamed Radio_Occultation_Support to Occultation_Supplement
        -  Removed ring_observation_id and source_pds3_id from all classes except Occultation_Supplement.
        -  Added Schematron rules to make some optional attributes required based on the value of 
           occultation type (e.g., dsn_station_number if occultation_type = radio, sub_stellar_ring_azimuth
           if occultation_type = stellar).
        -  Reordered some attributes in Occultation_Time_Series.
        -  Reordered some attributes in Occultation_Supplement.
      v1.5.0.0  2017-04-12
        -  Changed schema location URLs to https
        -  Updated to version 1.8.0.0 of IM.
        -  Revised definition of pds3_source_id
        -  Corrected the definition of sub_stellar_ring_azimuth
        -  Changed the name of the umbrella class from Occultation to Ring_Moon_Systems
        -  Added Time_Series_Direction 
      v1.5.1.0  2017-08-09
        -  corrected minor formating errors for a few enumerated values
        -  Reinstated the ring_plane attribute in the Occultation_Ring_Profile and Occultation_Time_Series classes.      
      v1.6.0.0  2019-03-06
        -  Updated to version 1.9.0.0 of IM.
        -  Added the Ring_Model class and numerous classes and attributes to support it.
        -  Added the Orbital_Elements class.
        -  ring_event_tdb - changed the enumeration flag to false
        -  added optional description attribute to several classes 
        -  added classes to support ring mosaics: Ring_Reprojection and Reprojection_Geometry.
        -  added several attributes to support ring mosaics.  
        - Added Display_Direction including pds:local_identifier_reference with a cardinality of [0,*].  
        - Added the class Ring_Spectrum
        - Added attributes
          - emission angle
          - ring_intercept_resolution
          - ring_longitude_observed_minus_subsolar 
          - reflectivity
        - Added an optional pds.local_identifier attribute to most classes.
        -  As an interim bandaid(?) pending repair of LDDTool, added several classes
           and attributes 'borrowed' from the geometry dictionary and removed the 
           geom. prefixes to those classes in this dictionary. The affected classes
           are:
                - Body_Ident_Base       
                - Frame_Ident_Base  (not used explicitly when geom is referenced)    
                - Reference_Frame_Ident 
                - Central_Body_Ident    
        - Added Uniformly_Sampled_Radius based on Uniformly_Sampled_Wavelength from the sp namespace 
        - Made the use of ring_observation_id optional.
        - @@@ Need schematron rule to ensure values for axis_name correspond to entries in Axis_Array.name 
      v1.7.0.0  2019-03-07
        - Updated to version 1.10.0.0 of IM.
        - Removed the Rings_Supplement class.
        - Removed the ring_observation_id attribute.
        - Removed pds:Internal_Reference from the Body_Ident_Base and Frame_Ident_Base classes.
        - Added a SChematron definition for a value in reference_type in pds:Internal_Reference in Uniformly_Sampled_Radius
      v1.8.0.0  2020-01-28
        - Updated to version 1.12.0.0 of IM.
        - Made Ring_Moon_Systems class the only xsi element.
        - removed the attribute source_pds3_id and spice_filename
        - removed milable from orbit_number and along_track_timing.
        - Added attributes fresnel_scale, projected_star_diameter, sigma_projected_star_diameter, fractional_error_star_counts, 
          time_constant_type, time_constant, sigma_time_constant.
        - All 7 of the preceding were added as optional attributes in the Occultation_Time_Series class
      v1.9.0.0  2020-01-31
        - Updated to version 1.13.0.0 of IM.
        - Add Units of Measure Type = Gmass to the gmass attribute.
      v1.10.0.0  2020-06-25
        - Updated to version 1.14.0.0 of IM.
        - Added the attributes: data_quality_index, ring_detected.
        - Revised the case of several attribute enumerated values from Title case to all lower case. The named rings of 
          Saturn are in title case while those of Uranus are lower case, consistent with normal usage by the community.
        - Added attributes min/max ring_longitude and observed_ring azimuth to Occultation_Time_Series.
        - Expanded definitions of highest and lowest detectable opacity. In each, set the minimum value to -1.0 which 
          indicates the signal was too poor to allow the calculation of the value.
      v1.11.0.0  2021-11-10
        - Defined the attributes and included in Occultation_Time_Series: 
          minimum_projected_sun_diameter, maximum_projected_sun_diameter, 
          sigma_projected_sun_diameter, average_unocculted_signal,
          lowest_detectable_normal_optical_depth, highest_detectable_normal_optical_depth,
        - Defined attributes antipated to be used as columns in data tables:
          observed_event_TDB_start_integration, observed_event_TDB_mid_integration,
          observed_event_TDB_stop_integration, ring_event_TDB_start_integration,
          ring_event_TDB_mid_integration, ring_event_TDB_stop_integration,
          ring_radius_start_integration, ring_radius_mid_integration, ring_radius_stop_integration,
          raw_total_counts,counts_per_second, transparency, normal_optical_depth,
          projected_sun_diameter. 
        - In Occultation_Ring_Profile and Occultation_Time_Series,changed the cardinality of 
          data_quality_index to [0,*].
        - Added to data_quality_index enumerated values to support solar occultations: B, F, R, U, X.
        - Revised the case of several attribute enumerated values to Title case.
        - Added the attribute: ring_detected.
        - Added attributes min/max ring_longitude and observed_ring azimuth to Occultation_Time_Series
    
   Last Modification Time 2021-11-10
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   body_spice_name
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The body_spice_name attribute is a NAIF-recognized string identifier for a physical object (spacecraft, planet, instrument transmitter, system barycenter, etc.), associated with the data. 

   name                   frame_spice_name
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The frame_spice_name attribute is a NAIF-recognized string identifier for a reference frame associated with the data. 

   name                   horizontal_display_axis
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The horizontal_display_axis attribute identifies, by name, the axis of an Array (or Array subclass) that is intended to be displayed in the horizontal or "sample" dimension on a display device. The value of this attribute must match the value of one, and only one, axis_name attribute in an Axis_Array class of the associated Array. 

   name                   horizontal_display_direction
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The horizontal_display_direction attribute specifies the direction across the screen of a display device that data along the horizontal axis of an Array is supposed to be displayed. 

   name                   vertical_display_axis
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The vertical_display_axis attribute identifies, by name, the axis of an Array (or Array subclass) that is intended to be displayed in the vertical or "line" dimension on a display device. The value of this attribute must match the value of one, and only one, axis_name attribute in an Axis_Array class of the associated Array. 

   name                   vertical_display_direction
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The vertical_display_direction attribute specifies the direction along the screen of a display device that data along the vertical axis of an Array is supposed to be displayed. 

   name                   orbit_number
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            orbit_number if present is the value assigned by the mission for the orbit number associated with the observation. Optional in labels of occultation observations and may be used multiple times. 

   name                   reflectivity
   version                1.19
   value data type        ASCII_Real
   description            reflectivity indicates I/F, a dimensionless standardized measure of reflectivity that is unity for a Lambertian surface viewed at normal incidence. 

   name                   minimum_reflectivity
   version                1.19
   value data type        ASCII_Real
   description            minimum_reflectivity indicates the smallest value of I/F within the data object. 

   name                   maximum_reflectivity
   version                1.19
   value data type        ASCII_Real
   description            maximum_reflectivity indicates the largest value of I/F within the data object. 

   name                   axis_name
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description             The axis_name attribute contains a string that matches the axis_name attribute in an axis_array class of an associated array object. 

   name                   sampling_interval_length
   version                1.19
   value data type        ASCII_Real
   description             The sampling_interval_length attribute provides the spacing of points, in units of length, at which data are sampled and at which a value for an instrument or data parameter is available. This sampling interval can be either the original (raw) sampling or the result of some resampling process. 
   unit of measure type   Units_of_Length

   name                   sampling_base
   version                1.19
   value data type        ASCII_Real
   description             The sampling_base attribute indicates the numeric base of the associated logarithmic or exponential sampling interval. 

   name                   sampling_scale
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description             The sampling_scale attribute indicates the type of scale that applies to the sample interval increments. It must have a value of either Linear, Logarithmic or Exponential. 

   name                   first_ring_radius
   version                1.19
   value data type        ASCII_Real
   description             The first_ring_radius attribute provides the value of the first increment along the radius axis of an array given in units of length. 
   unit of measure type   Units_of_Length

   name                   last_ring_radius
   version                1.19
   value data type        ASCII_Real
   description             The last_ring_radius attribute provides the value of the last increment along the radius axis of an array given in units of length. 
   unit of measure type   Units_of_Length

   name                   sclk_start_time
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            sclk_start_time is the value of the spacecraft clock corresponding to the start_date_time given in the label. 

   name                   sclk_stop_time
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            sclk_stop_time is the value of the spacecraft clock corresponding to the stop_date_time given in the label. 

   name                   reference_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            reference_time_utc provides a date and time in UTC format. Given in a label when time values in a table are given as elapsed seconds offset from a reference time. Unless there are compelling reasons to do otherwise, reference_time_utc should correspond to the start of a day. Required anytime a table field is given relative to a specific date and time other than when Barycentric Dynamical Time is used (e.g., observed_event_tdb). 
   unit of measure type   Units_of_Time

   name                   observed_event_time
   version                1.0
   value data type        ASCII_Real
   description            observed_event_time indicates the instant at which photons were received at the instrument. As a field in an occultation profile table, it is given in numeric seconds as an offset from the specified UTC reference time. The reference time is preferably the start of a day. In a label the corresponding time interval end point values are given by the required start_date_time_utc and stop_date_time_utc attributes in the Time_Coordinates class. At least one of either observed_event_time or observed_event_tdb, must be a table field for occultation data. Both may be used. observed_event_time is equivalent to spacecraft_event_time for spacecraft data and to earth_received_time for Earth-based data. It is always the photon arrival time, so in this regard we treat typical spacecraft radio occultation data as Earth-based, referring to the time at the DSN receiving station. For an uplink radio occultation, this is the spacecraft event time. Note: For occultation data, PDS prefers year-month-day format for dates rather than year plus day-of-year format. However, either format is permitted. 
   unit of measure type   Units_of_Time

   name                   maximum_observed_event_time
   version                1.19
   value data type        ASCII_Real
   description            maximum_observed_event_time gives the largest value for observed_event_time in the associated data file. It is given in numeric seconds as an offset from the specified UTC reference time. maximum_observed_event_time is optional in labels since the data file time interval end point values are given by the required start_date_time_utc and stop_date_time_utc attributes in the Time_Coordinates class. 
   unit of measure type   Units_of_Time

   name                   minimum_observed_event_time
   version                1.19
   value data type        ASCII_Real
   description            minimum_observed_event_time gives the smallest value for observed_event_time in the associated data file. It is given in numeric seconds as an offset from the specified UTC reference time. minimum_observed_event_time is optional in labels since the data file time interval end point values are given by the required start_date_time_utc and stop_date_time_utc attributes in the Time_Coordinates class. 
   unit of measure type   Units_of_Time

   name                   observed_event_tdb
   version                1.0
   value data type        ASCII_Real
   description            observed_event_tdb indicates the instant at which photons were received at the instrument. It is represented in the 'Barycentric Dynamical Time' system, as a number of elapsed seconds since the J2000 epoch. This is consistent with the definition of 'ephemeris time' as used in the SPICE toolkit. In a label the corresponding values are given by the optional start_observed_event_tdb and stop_observed_event_tdb attributes. At least one of either observed_event_time or observed_event_tdb, must be a table field for occultation data. Both may be used. observed_event_time is equivalent to spacecraft_event_time for spacecraft data and to earth_received_time for Earth-based data. It is always the photon arrival time, so in this regard we treat typical spacecraft radio occultation data as Earth-based, referring to the time at the DSN receiving station. For an uplink radio occultation, this is the spacecraft event time. 
   unit of measure type   Units_of_Time

   name                   observed_event_start_tdb
   version                1.19
   value data type        ASCII_Real
   description            observed_event_start_tdb indicates the value for earliest time in the described data, and is given in elapsed seconds since the J2000 epoch. Optional in labels; not intended for use as a table field.
   unit of measure type   Units_of_Time

   name                   observed_event_stop_tdb
   version                1.19
   value data type        ASCII_Real
   description            observed_event_stop_tdb indicates the value for latest time in the described data, and is given in elapsed seconds since the J2000 epoch. Optional in labels; not intended for use as a table field. 
   unit of measure type   Units_of_Time

   name                   observed_event_time_utc
   version                1.0
   value data type        ASCII_Real
   description            This attribute is intended to be used as a column in a table. observed_event_time_utc indicates the UTC time corresponding to the instant at which photons were received at the instrument. In a label the corresponding values may be given by the optional start_observed_event_utc and stop_observed_event_utc attributes (or the corresponding values using Barycentric Dynamical Time, _tdb). At least one of either observed_event_time_utc or observed_event_tdb, must be a table field for occultation data. Both may be used. observed_event_time is equivalent to spacecraft_event_time for spacecraft data and to earth_received_time for Earth-based data. It is always the photon arrival time, so in this regard we treat typical spacecraft radio occultation data as Earth-based, referring to the time at the DSN receiving station. For an uplink radio occultation, this is the spacecraft event time. 
   unit of measure type   Units_of_Time

   name                   observed_event_start_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            observed_event_start_time_utc indicates the UTC value for earliest time in the described data. It is part of a start/stop pair. If one of observed_event_start_time_utc and observed_event_stop_time_utc is used, both must be used. 

   name                   observed_event_stop_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            observed_event_stop_time_utc indicates the UTC value for latest time in the described data. It is part of a start/stop pair. If one of observed_event_start_time_utc and observed_event_stop_time_utc is used, both must be used. 

   name                   spacecraft_event_time
   version                1.0
   value data type        ASCII_Real
   description            spacecraft_event_time indicates the instant at which an event occurred at the spacecraft, e.g., the arrival or departure of a photon. Required table field for radio occultation data, but not used in stellar occultation data. The time is given in numeric seconds as an offset from the specified UTC reference time. The reference time is preferably the start of a day, and is required to be given in the label using the attribute reference_time_utc. Additionally, in radio occultation labels the corresponding time interval end point values are given by the required start_spacecraft_event_time_utc and stop_spacecraft_event_time_utc attributes. 
   unit of measure type   Units_of_Time

   name                   spacecraft_event_start_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            spacecraft_event_start_time_utc gives the UTC time corresponding to the earliest time given by spacecraft_event_time in the data table. However, while spacecraft_event_time is given as seconds offset from a reference time, spacecraft_event_start_time_utc is given as a UTC date time. Required in the label for radio occultation data. Not used for stellar occultations. 
   unit of measure type   Units_of_Time

   name                   spacecraft_event_stop_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            spacecraft_event_stop_time_utc gives the UTC time corresponding to the latest time given by spacecraft_event_time in the data table. However, while spacecraft_event_time is given as seconds offset from a reference time, spacecraft_event_stop_time_utc is given as a UTC date time. Required in the label for radio occultation data. Not used for stellar occultations. 
   unit of measure type   Units_of_Time

   name                   earth_received_time
   version                1.0
   value data type        ASCII_Real
   description            earth_received_time provides the time at which telemetry or other photons were received on Earth. Intended to be used as a table field which is optional for stellar occultations, and is not used for radio occultation data (one of either observed_event_time or observed_event_tdb is used instead). earth_received_time is given in numeric seconds as an offset from the specified UTC reference time. The reference time is preferably the start of a day, and is required to be given in the label using the attribute reference_time_utc. This is equivalent to OBSERVED_EVENT_TIME for radio occultations. It is an optional table field for stellar occultations and is not used for radio occultations. When earth_received_time is used, the attribute reference_time_utc is required in the label. 
   unit of measure type   Units_of_Time

   name                   earth_received_start_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            earth_received_start_time_utc gives the UTC time corresponding to the earliest time for the data product at which telemetry or other photons were received on Earth. Optional for occultation data. 
   unit of measure type   Units_of_Time

   name                   earth_received_stop_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            earth_received_stop_time_utc gives the UTC time corresponding to the latest time for the data product at which telemetry or other photons were received on Earth. Optional for occultation data. 
   unit of measure type   Units_of_Time

   name                   ring_event_time
   version                1.0
   value data type        ASCII_Real
   description            ring_event_time indicates the instant at which photons associated with a particular ring observation intercepted the ring plane. This time is earlier than the associated observed_event_time by an amount equal to the light travel time. ring_event_time is a required table field for ring occultation data. The time is given in numeric seconds as an offset from the specified UTC reference time. The reference time is preferably the start of a day, and is required to be given in the label using the attribute reference_time_utc. One of ring_event_time or ring_event_tdb is a required table field for all ring occultations. One of ring_event_time or ring_event_tdb is a required table field for all ring occultations. Both may be used. If ring_event_time is used, the attribute reference_time_utc is required in the label. 
   unit of measure type   Units_of_Time

   name                   ring_event_start_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            ring_event_start_time_utc gives the UTC time corresponding to the earliest time given by ring_event_time or ring_event_tdb in the data table. ring_event_start_time_utc is required for all ring occultation data. ring_event_start_time_utc is required label attribute for all ring occultation data. 
   unit of measure type   Units_of_Time

   name                   ring_event_stop_time_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            ring_event_stop_time_utc gives the UTC time corresponding to the latest time given by ring_event_time or ring_event_tdb in the data table. ring_event_stop_time_utc is required for all ring occultation data. ring_event_stop_time_utc is required label attribute for all ring occultation data. 
   unit of measure type   Units_of_Time

   name                   ring_event_tdb
   version                1.0
   value data type        ASCII_Real
   description            ring_event_tdb indicates the instant at which photons associated with a particular ring observation left the ring plane. This time is earlier than the associated observed_event_tbd by an amount equal to the light travel time. ring_event_tdb is represented in the 'Barycentric Dynamical Time' system, as a number of elapsed seconds since the J2000 epoch. This is consistent with the definition of 'ephemeris time' as used in the SPICE toolkit. One of ring_event_time or ring_event_tdb is a required table field for all ring occultations. Both may be used. 
   unit of measure type   Units_of_Time

   name                   ring_event_start_tdb
   version                1.19
   value data type        ASCII_Real
   description            ring_event_start_tdb indicates the value for earliest time in the described data, and is given in ring_event_tdb format. Optional in labels; not intended for use as a table field. 
   unit of measure type   Units_of_Time

   name                   ring_event_stop_tdb
   version                1.19
   value data type        ASCII_Real
   description            ring_event_stop_tdb indicates the value for latest time in the described data, and is given in ring_event_tdb format. Optional in labels; not intended for use as a table field. 
   unit of measure type   Units_of_Time

   name                   along_track_timing_offset
   version                1.19
   value data type        ASCII_Real
   description            along_track_timing_offset is a timing offset to the along track spacecraft position. It is the value that minimizes differences in radii of matching circular ring features observed on the ingress and egress sides of the occultation track. Optional in labels for radio occultation. 
   unit of measure type   Units_of_Time

   name                   data_quality_index
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            data_quality_index provides a more precise subjective assessment by the data provider of the quality of the observed/predicted ring occultation. Possible values are:. 

   name                   data_quality_score
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            data_quality_score indicates the overall quality of the data, based on a subjective evaluation by the data provider. Required in labels of ring occultation radial profiles. Normally not intended as a value for a table field. 

   name                   ring_detected
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The ring_detected attribute is a yes-or-no flag that indicates whether a specific ring has been detected. Typically used in radial profiles of a single ring. 
   minimum characters     1
   maximum characters     1

   name                   occultation_type
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            occultation_type distinguishes between three types of occultation experiments: Stellar, Solar, or Radio. Stellar occultations involve observing a star as a targeted ring or body passes in front, as seen from either a spacecraft or Earth-based observatory. Solar occultations are similar to stellar occultations except that the Sun is used in place of a star. Radio occultations typically involve observing the continuous-wave radio transmissions from a spacecraft as it passes behind the target as seen from a radio telescope on Earth or another spacecraft. Required in labels of occultation observations. Normally not intended as a value for a table field. 

   name                   planetary_occultation_flag
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The planetary_occultation_flag is a yes-or-no flag that indicates whether a occultation track also intersects the planet. Required in labels of ring occultation observations. Normally not intended as a value for a table field. 
   minimum characters     1
   maximum characters     1

   name                   occultation_direction
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            occultation_direction indicates the direction of an occultation track. This refers to the observed occultation track overall, not to the subset that might appear in a particular file (e.g., if an occultation includes both ingress and egress tracks, the value for occultation_direction will be both in the data products for each occultation profile. Permitted values are 'ingress', 'egress', 'both', and 'multiple'. The value 'multiple' is used where the occultation track is not monotonic over relatively short time scales. Generally only used for some Hubble-based occultations. May be appropriate for extremely long duration occultations of a high proper motion star (e.g., u36). Required in labels of ring occultation observations. Not intended as a value for a table field. 

   name                   star_name
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            star_name provides the identifying name of star, including the catalog name if necessary. Examples include 'sigma Sgr' and 'SAO 123456' (for star number 123456 in the Smithsonian Astrophysical Observatory catalog). Use 'Sun' for solar occultations. Required in labels for stellar and solar occultations. Not used for radio occultations. 

   name                   radial_resolution
   version                1.19
   value data type        ASCII_Real
   description            radial_resolution indicates the nominal radial distance over which changes in ring properties can be detected within a data product. Note: this value may be larger than the radial_sampling_interval value, because a data product can be over-sampled. Required in labels if the value is fixed, as it is for stellar occultations. If the value varies, the corresponding minimum and maximum attributes must be used instead. Not intended to be used as a table field. 
   unit of measure type   Units_of_Length

   name                   minimum_radial_resolution
   version                1.19
   value data type        ASCII_Real
   description            minimum_radial_resolution indicates the minimum radial distance over which changes in ring properties can be detected within a data product. Note: this value may be larger than the radial_sampling_interval value, because a data product can be over-sampled. If the value of radial resolution varies, the minimum and maximum radial resolution attributes are required in labels. Not intended to be used as a table field. 
   unit of measure type   Units_of_Length

   name                   maximum_radial_resolution
   version                1.19
   value data type        ASCII_Real
   description            maximum_radial_resolution indicates the maximum radial distance over which changes in ring properties can be detected within a data product. Note: this value may be larger than the radial_sampling_interval value, because a data product can be over-sampled. If the value of radial resolution varies, the minimum and maximum radial resolution attributes are required in labels. Not intended to be used as a table field. 
   unit of measure type   Units_of_Length

   name                   ring_intercept_resolution
   version                1.19
   value data type        ASCII_Real
   description            ring_intercept_resolution is the size of edge of a pixel at the distance of the ring intercept point. If the pixel shape is not square, it is defined by the smaller of the two edges. Unlike the quantity ‘radial resolution’, these values are not projected into the ring plane. 
   unit of measure type   Units_of_Length

   name                   minimum_ring_intercept_resolution
   version                1.19
   value data type        ASCII_Real
   description            minimum_ring_intercept_resolution indicates the smallest value for ring_intercept_resolution in the data product. 
   unit of measure type   Units_of_Length

   name                   maximum_ring_intercept_resolution
   version                1.19
   value data type        ASCII_Real
   description            maximum_ring_intercept_resolution indicates the largest value for ring_intercept_resolution in the data product. 
   unit of measure type   Units_of_Length

   name                   radial_sampling_interval
   version                1.19
   value data type        ASCII_Real
   description            radial_sampling_interval indicates the radial spacing between consecutive points in a ring profile. In practice, this may be somewhat smaller than the radial_resolution because a profile may be over-sampled. Required in labels if the value is fixed. If the value varies, the corresponding minimum and and maximum attributes must be used instead. Not intended to be used as a table field. 
   unit of measure type   Units_of_Length

   name                   minimum_radial_sampling_interval
   version                1.19
   value data type        ASCII_Real
   description            minimum_radial_sampling_interval indicates the smallest radial spacing between consecutive points in a ring profile. In practice, this may be somewhat smaller than the radial_resolution because a profile may be over-sampled. If the value of radial_sampling_interval varies, the minimum and maximum attributes are required in labels. Not intended to be used as a table field. 
   unit of measure type   Units_of_Length

   name                   maximum_radial_sampling_interval
   version                1.19
   value data type        ASCII_Real
   description            maximum_radial_sampling_interval indicates the largest radial spacing between consecutive points in a ring profile. In practice, this may be somewhat smaller than the radial_resolution because a profile may be over-sampled. If the value of radial_sampling_interval varies, the minimum and maximum attributes are required in labels. Not intended to be used as a table field. 
   unit of measure type   Units_of_Length

   name                   ring_plane
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            ring_plane indicates the plane upon which parameters such as ring_radius are based. Possible values for the Saturn ring system are 'Equator', 'A', 'B', 'C', 'D', 'E', 'F', 'G', 'Phoebe'. For the Uranus ring system values are 'Equator', 'six', 'five', 'four', 'alpha', 'beta', 'eta', 'gamma', 'delta', 'lambda','epsilon',nu, mu. An additional value, 'individual' is also defined. Note that the named rings of Saturn are in title case while those of Uranus are lower case, consistent with normal usage by the community. Required in labels of ring occultation observations. 

   name                   ring_profile_direction
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            ring_profile_direction indicates the radial direction of a ring occultation within a particular data product. Possible values are 'Ingress', 'Egress', or 'Multiple'. The value 'Multiple' is used where the occultation track is not monotonic over relatively short time scales. Generally only used for some Hubble-based occultations. May be appropriate for extremely long duration occultations of a high proper motion star (e.g., u36). Required in labels of ring occultation observations. Not intended as a value for a table field. 

   name                   time_series_direction
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            time_series_direction indicates the direction the occultation proceeds through the target within a particular data product. Possible values are 'Ingress', 'Egress', 'Both' or 'Multiple'. The value 'Multiple' is used where the occultation track is not monotonic over relatively short time scales. Generally only used for some Hubble-based occultations. May be appropriate for extremely long duration occultations of a high proper motion star (e.g., u36). Not intended as a value for a table field. 

   name                   normal_optical_depth
   version                1.0
   value data type        ASCII_Real
   description            normal_optical_depth is the ratio of incident to transmitted radiant power corrected for background_signal and for the value of observed_ring_elevation (the viewing angle). Normal optical depth is defined as the observed_optical_depth times the sine of observed_ring_elevation. Typically negative values are used to indicate the signal was too poor to allow the calculation of the value. 
   minimum value          -2000

   name                   lowest_detectable_normal_optical_depth
   version                1.19
   value data type        ASCII_Real
   description            lowest_detectable_normal_optical_depth gives the theoretical lowest possible normal optical depth that can be detected in the observation based on the background signal and unocculted signal measurements. 

   name                   highest_detectable_normal_optical_depth
   version                1.19
   value data type        ASCII_Real
   description            highest_detectable_normal_optical_depth gives the theoretical highest possible normal optical depth that can be detected in the observation based on the background signal and unocculted signal measurements. 

   name                   highest_detectable_opacity
   version                1.19
   value data type        ASCII_Real
   description            highest_detectable_opacity indicates the sensitivity of a ring occultation data set to nearly opaque rings. It specifies the rough value for the largest normal ring opacity that can be detected in the data at the resolution provided, incorporating both statistical effects and calibration uncertainties. -1.0 indicates the signal was too poor to allow the calculation of the value. Strongly recommended in labels of ring occultation observations. Not intended as a value for a table field. 
   minimum value          -1

   name                   lowest_detectable_opacity
   version                1.19
   value data type        ASCII_Real
   description            lowest_detectable_opacity indicates the sensitivity of a ring occultation data set to nearly opaque rings. It specifies the rough value for the smallest normal ring opacity that can be detected in the data at the resolution provided, incorporating both statistical effects and calibration uncertainties. -1.0 indicates the signal was too poor to allow the calculation of the value. Strongly recommended in labels of ring occultation observations. Not intended as a value for a table field. 
   minimum value          -1

   name                   background_signal
   version                1.19
   value data type        ASCII_Real
   description            background_signal indicates the anticipated signal (in counts, counts per second, or other specified units) received when no occulted source signal reaches the detector. This is the signal level that indicates an opaque ring. Strongly recommended in labels of ring occultation observations if the value is constant, or strongly recommended to be used as a field in the data table if the value is not constant. Normally not used for radio occultations. 

   name                   stellar_signal_level
   version                1.0
   value data type        ASCII_Real
   description            stellar_signal_level indicates the anticipated signal from an un-occulted star, in the absence of any background signal. This is the signal level that defines the difference between a transparent ring and an opaque ring. Strongly recommended in labels of ring stellar occultation observations if the value is constant. For stellar occultations, if the value is not constant, strongly recommended to be used as a field in the data table. Not used for radio occultations. 

   name                   average_unocculted_signal
   version                1.19
   value data type        ASCII_Real
   description            average_unocculted_signal indicates the average of the signal in counts/second received from outside the rings or from nominally transparent regions of the rings after subtraction of background signal. Strongly recommended in labels of ring solar occultation observations if the value is constant. For solar occultations, if the value is not constant, strongly recommended to be used as a field in the data table. Not used for radio occultations. 

   name                   ring_radius
   version                1.0
   value data type        ASCII_Real
   description            ring_radius indicates a radial location within a planetary ring system. Radii are measured from the center of mass of the planet along the nominal ring plane. Units are km and are always positive. Required to be the first field in ring occultation profiles. Data are always organized with ring radius increasing. In labels, the min and max attributes are required. 
   unit of measure type   Units_of_Length

   name                   minimum_ring_radius
   version                1.19
   value data type        ASCII_Real
   description            minimum_ring_radius indicates the smallest ring radius value in the data table. Units are km and are always positive. Required in label files for ring occultation data. 
   unit of measure type   Units_of_Length

   name                   maximum_ring_radius
   version                1.19
   value data type        ASCII_Real
   description            maximum_ring_radius indicates the largest ring radius value in the data table. Units are km and are always positive. Required in label files for ring occultation data. 
   unit of measure type   Units_of_Length

   name                   ring_longitude
   version                1.19
   value data type        ASCII_Real
   description            ring_longitude specifies the inertial longitude of a ring feature relative to the prime meridian. In planetary ring systems, the prime meridian is the ascending node of the planet's invariable plane on the Earth's mean equator of J2000. Longitudes are measured in the direction of orbital motion along the planet's invariable plane to the ring's ascending node, and thence along the ring plane. Values range from 0 to 360 in units of degrees. Note: The invariable plane of a planet is equivalent to its equatorial plane for every ringed planet except Neptune. Required to be the second field in ring occultation profiles. In labels, the min and max attributes are required. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   minimum_ring_longitude
   version                1.19
   value data type        ASCII_Real
   description            minimum_ring_longitude specifes one boundary for the ring longitude range in the data; normally the smallest value. However, for ranges that cross the prime meridian, the minimum ring longitude will have a value greater than the maximum ring longitude. Values range from 0 to 360 in units of degrees. Required in label files for ring occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   maximum_ring_longitude
   version                1.19
   value data type        ASCII_Real
   description            maximum_ring_longitude specifies one boundary for the ring longitude range in the data; normally the largest value. However, for ranges that cross the prime meridian, the maximum ring longitude will have a value less than the minimum ring longitude. Values range from 0 to 360 in units of degrees. Required in label files for ring occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   ring_longitude_observed_minus_subsolar
   version                1.19
   value data type        ASCII_Real
   description            ring_longitude_observed_minus_subsolar providees the difference between the inertial ring longitude of the observation and inertial ring longitude of the sub-solar point. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   minimum_ring_longitude_observed_minus_subsolar
   version                1.19
   value data type        ASCII_Real
   description            minimum_ring_longitude_observed_minus_subsolar specifes smallest separation in ring longitude between the observation and the sub-solar point. Required in label files for ring occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   maximum_ring_longitude_observed_minus_subsolar
   version                1.19
   value data type        ASCII_Real
   description            maximum_ring_longitude_observed_minus_sub-solar specifes smallest separation in ring longitude between the observation and the subsolar point. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   observed_ring_elevation
   version                1.19
   value data type        ASCII_Real
   description            observed_ring_elevation is an angle measured at a point in the ring plane, starting from the ring plane to the direction of a photon heading to the observer. This angle is positive on the side of the ring plane defined by positive angular momentum, and negative on the opposite side. Values range from -90 to +90 in units of degrees. This angle is constant for stellar occultations, but may vary significantly during radio occultations. Note: The direction of positive angular momentum points toward the IAU-defined north side of the ring plane for Jupiter, Saturn and Neptune, but IAU-defined south side of the ring plane for Uranus. Required in the label if the value is constant for the observation. If the angle varies for the observation, the min and max attributes are required in the label, and observed_ring_elevation is strongly recommended as a field in the data table. The above definition of observed_ring_elevation is equivalent to the most common usage of the term 'ring open angle', B. 
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   minimum_observed_ring_elevation
   version                1.19
   value data type        ASCII_Real
   description            minimum_observed_ring_elevation specifes the smallest value for observed_ring_elevation in the data file. Only used if the value is not constant over the observation. Values range from -90 to +90 in units of degrees. Not intended for use in the data file. 
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   maximum_observed_ring_elevation
   version                1.19
   value data type        ASCII_Real
   description            maximum_observed_ring_elevation specifes the largest value for observed_ring_elevation in the data file. Only used if the value is not constant over the observation. Values range from -90 to +90 in units of degrees. Not intended for use in the data file. 
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   mean_observed_ring_elevation
   version                1.19
   value data type        ASCII_Real
   description            mean_observed_ring_elevation specifes the mean value for observed_ring_elevation in the data file. 
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   emission_angle
   version                1.19
   value data type        ASCII_Real
   description            The emission_angle element provides the value of the angle between the surface normal vector at the intercept point and a vector from the intercept point to the spacecraft. Higher values of emission_angle indicate more oblique viewing of the target. The emission_angle varies from 0 degrees when the spacecraft is viewing the subspacecraft point (nadir viewing) to 90 degrees when the intercept is tangent to the surface of the target body, values in the range of 90 to 180 degrees are possible for ring data. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   minimum_emission_angle
   version                1.19
   value data type        ASCII_Real
   description            The minimum_emission_angle attribute provides the smallest value during the observation for the emission angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   maximum_emission_angle
   version                1.19
   value data type        ASCII_Real
   description            The maximum_emission_angle element provides the largest value during the observation for the emission angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   incidence_angle
   version                1.19
   value data type        ASCII_Real
   description            The incidence_angle element provides a measure of the lighting condition at the intercept point. Incidence angle is the angle the surface normal vector at the intercept point and a vector from the intercept point to the sun. The incidence_angle varies from 0 degrees when the intercept point coincides with the subsolar point to 90 degrees when the intercept is tangent to the surface of the target body, values in the range of 90 to 180 degrees are possible for ring data. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   minimum_incidence_angle
   version                1.19
   value data type        ASCII_Real
   description            The minimum_incidence_angle attribute provides the smallest value during the observation for the incidence angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   maximum_incidence_angle
   version                1.19
   value data type        ASCII_Real
   description            The maximum_incidence_angle element provides the largest value during the observation for the incidence angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   light_source_incidence_angle
   version                1.19
   value data type        ASCII_Real
   description            light_source_incidence_angle is an angle measured from the local surface normal vector to the direction of a photon arriving from the light source. For rings, the normal vector is that on the same side of the rings as the light source, so values always range between 0 and 90 in units of degrees. The value is always equal to 90 - | observed_ring_elevation | This will enable users to perform database searches based on the effective ring opening angle when they are not concerned about the distinction between north-side and southside viewpoints. We have included the 'light source' prefix to the term so that this quantity is not confused with 'incidence angle', a term that is generally associated with sunlight rather than stars or radio transmitters. Required in the label if the value is constant for the observation. If the angle varies for the observation, the min and max attributes are required in the label. Optional as a field in the data table. 
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   minimum_light_source_incidence_angle
   version                1.19
   value data type        ASCII_Real
   description            minimum_light_source_incidence_angle specifes the smallest value for light_source_incidence_angle in the observation. Only used if the value is not constant over the observation. Values range from 0 to +90 in units of degrees. Not intended for use in the data file. 
   minimum value          0
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   maximum_light_source_incidence_angle
   version                1.19
   value data type        ASCII_Real
   description            maximum_light_source_incidence_angle specifes the largest value for light_source_incidence_angle in the observation. Only used if the value is not constant over the observation. Values range from 0 to +90 in units of degrees. Not intended for use in the data file. 
   minimum value          0
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   phase_angle
   version                1.0
   value data type        ASCII_Real
   description            The phase_angle element provides a measure of the relationship between the instrument viewing position and incident illumination (such as solar light). Phase angle is measured at the target; it is the angle between a vector to the illumination source and a vector to the instrument. If not specfied, the target is assumed to be at the center of the instrument field of view. If illumination is from behind the instrument, phase_angle will be small. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   minimum_phase_angle
   version                1.19
   value data type        ASCII_Real
   description            The minimum_phase_angle attribute provides the smallest value during the observation for the phase angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   maximum_phase_angle
   version                1.19
   value data type        ASCII_Real
   description            The maximum_phase_angle element provides the largest value during the observation for the phase angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   mean_phase_angle
   version                1.19
   value data type        ASCII_Real
   description            The mean_phase_angle element provides the mean value during the observation for the phase angle at the target. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   observed_ring_azimuth
   version                1.0
   value data type        ASCII_Real
   description            observed_ring_azimuth is an angle measured at a point in the ring plane, starting from the direction of a photon heading to the observer, and ending at the direction of a local radial vector. This angle is projected into the ring plane and measured in the prograde direction. Note that, as seen from the observer, it equals 90 degrees along the right ansa and 270 degrees along the left ansa. Values range from 0 to 360 in units of degrees. Required to be the third field in ring occultation profiles. In labels, the min and max attributes are required. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   minimum_observed_ring_azimuth
   version                1.19
   value data type        ASCII_Real
   description            minimum_observed_ring_azimuth specifes the smallest value for observed_ring_azimuth in the data file. Values range from 0 to 360 in units of degrees. Required in label files for ring occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   maximum_observed_ring_azimuth
   version                1.19
   value data type        ASCII_Real
   description            maximum_observed_ring_azimuth specifes the largest value for observed_ring_azimuth in the data file. Values range from 0 to 360 in units of degrees. Required in label files for ring occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   sub_stellar_ring_azimuth
   version                1.19
   value data type        ASCII_Real
   description            sub_stellar_ring_azimuth is an angle measured at a point in the ring plane, starting from the direction of a photon arriving from a star, and ending at the direction of a local radial vector. This angle is projected into the ring plane and measured in the prograde direction. Values range from 0 to 360 in units of degrees. For stellar occultation data, this angle is equal to (observed_ring_azimuth + 180) mod 360. It is available only for backward compatibility with previously published Cassini UVIS occultation data analysis; observed_ring_azimuth is the preferred quantity for archiving. sub_stellar_ring_azimuth is an optional data table field for Cassini UVIS occultation data; not recommended for other occultation data. In a label, the min and max variation attributes are optional for Cassini UVIS occultation data; not recommended for other occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   minimum_sub_stellar_ring_azimuth
   version                1.0
   value data type        ASCII_Real
   description            minimum_sub_stellar_ring_azimuth specifes the smallest value for sub_stellar_ring_azimuth in the data file. Values range from 0 to 360 in units of degrees. Optional label attribute for Cassini UVIS occultation data; not used for other occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   maximum_sub_stellar_ring_azimuth
   version                1.0
   value data type        ASCII_Real
   description            maximum_sub_stellar_ring_azimuth specifes the largest value for sub_stellar_ring_azimuth in the data file. Values range from 0 to 360 in units of degrees. Optional label attribute for Cassini UVIS occultation data; not used for other occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   sub_stellar_clock_angle
   version                1.19
   value data type        ASCII_Real
   description            sub_stellar_clock_angle is an angle measured at a point in the ring plane, from the direction toward a star to the local radial direction. This angle is projected into the ring plane and measured in the clockwise (retrograde) direction. Equivalently, this is the prograde angle from the local radial direction to the direction toward the star. For stellar occultation data, this angle is equal to (180 - OBSERVED_RING_AZIMUTH) mod 360. It is available only for backward compatibility with previously published Cassini VIMS occultation data analysis; observed_ring_azimuth is the preferred quantity for archiving. sub_stellar_clock_angle is an optional data table field for Cassini VIMS occultation data; not recommended for other occultation data. In a label, the min and max variation attributes are optional for Cassini VIMS occultation data; not recommended for other occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   minimum_sub_stellar_clock_angle
   version                1.0
   value data type        ASCII_Real
   description            minimum_sub_stellar_clock_angle specifes the smallest value for sub_stellar_clock_angle in the data file. Values range from 0 to 360 in units of degrees. Optional label attribute for Cassini VIMS occultation data; not used for other occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   maximum_sub_stellar_clock_angle
   version                1.0
   value data type        ASCII_Real
   description            maximum_sub_stellar_clock_angle specifes the largest value for sub_stellar_clock_angle in the data file. Values range from 0 to 360 in units of degrees. Optional label attribute for Cassini VIMS occultation data; not used for other occultation data. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   wavelength
   version                1.19
   value data type        ASCII_Real
   description            wavelength of the observation. Optional in labels. If the observation is over a wavelength range, use the corresponding minimum and maximum attributes instead. 
   unit of measure type   Units_of_Length

   name                   minimum_wavelength
   version                1.19
   value data type        ASCII_Real
   description            minimum_wavelength is the smallest wavelength used in the observation. Optional in labels. Used with maximum_wavelength when the observation is over a wavelength range. 
   unit of measure type   Units_of_Length

   name                   maximum_wavelength
   version                1.19
   value data type        ASCII_Real
   description            maximum_wavelength is the largest wavelength used in the observation. Optional in labels. Used with minimum_wavelength when the observation is over a wavelength range. 
   unit of measure type   Units_of_Length

   name                   dsn_station_number
   version                1.19
   value data type        ASCII_Integer
   description            dsn_station_number identifies the receiving DSN station. Required in labels for radio occultations; not used for stellar occultations. Nillable in which case the nil_reason should be 'inapplicable'. 
   nillable               true

   name                   frequency_band
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description             The frequency_band attribute provides the one or two letter identifier for the frequency band associated with radio occultation data. Required in labels for radio occultations; not used for stellar occultations. 

   name                   fresnel_scale
   version                1.19
   value data type        ASCII_Real
   description            fresnel_scale is sqrt(lambda * D/2), where lambda is the central wavelength of the observation and D is the average distance between the observer and the occulting ring. This is an average value for the entire occultation and is a measure of the limit on the radial resolution of ring structure due to diffraction. Note that the actual overall resolution is affected as well by the projected diameter of the occulted star and the instrumental time constant, if any. 
   unit of measure type   Units_of_Length

   name                   projected_star_diameter
   version                1.19
   value data type        ASCII_Real
   description            projected_star_diameter provides the projected angular diameter of the occulted star, from observer to occulting object. 
   unit of measure type   Units_of_Length

   name                   sigma_projected_star_diameter
   version                1.19
   value data type        ASCII_Real
   description            sigma_projected_star_diameter indicates the uncertainty (1-sigma) in the projected_star_diameter. 
   unit of measure type   Units_of_Length

   name                   fractional_error_star_counts
   version                1.19
   value data type        ASCII_Real
   description            fractional_error_star_counts indicates the fractional error (1-sigma) in star counts used for square-well model fit. 

   name                   time_constant_type
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            time_constant_type distinguishes between three types of instrumental time constant assumed in a square-well model. This attribute is required if the time_constant attribute is present. 

   name                   time_constant
   version                1.19
   value data type        ASCII_Real
   description            time_constant indicates the instrumental time constant of the detector. See Eq. 9 Elliot et al. (1984) Astron. J. 1587-1603. If this attribute is used them the attribute time_constant_type also must be present. 
   unit of measure type   Units_of_Time

   name                   sigma_time_constant
   version                1.19
   value data type        ASCII_Real
   description            sigma_time_constant indicates the uncertainty in the time_constant. See Eq. 9 Elliot et al. (1984) Astron. J. 1587-1603. If this attribute is used them the attribute time_constant also must be present. 
   unit of measure type   Units_of_Time

   name                   projected_sun_diameter
   version                1.0
   value data type        ASCII_Real
   description            projected_sun_diameter provides the diameter in kilometers of the sun projected onto the ring plane radius based on the line of sight from the observer to the ring plane at the start of the integration assuming the sun subtends a circular disk with an angular size based on the distance of the central body from the sun. 
   unit of measure type   Units_of_Length

   name                   minimum_projected_sun_diameter
   version                1.19
   value data type        ASCII_Real
   description            minimum_projected_sun_diameter provides the smallest value of projected_sun_diameter in the obsevation. 
   unit of measure type   Units_of_Length

   name                   maximum_projected_sun_diameter
   version                1.19
   value data type        ASCII_Real
   description            maximum_projected_sun_diameter provides the largest value of projected_sun_diameter in the obsevation. 
   unit of measure type   Units_of_Length

   name                   sigma_projected_sun_diameter
   version                1.19
   value data type        ASCII_Real
   description            sigma_projected_sun_diameter indicates the Standard deviation (1-sigma) of projected_sun_diameter in the observation. 
   unit of measure type   Units_of_Length

   name                   pole_right_ascension_angle
   version                1.19
   value data type        ASCII_Real
   description            The right ascension (RA) of the pole of the specified body, given in angular measurements. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   pole_right_ascension_angle_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty of the right ascension (RA) of the pole of the specified body, given in angular measurements. 
   unit of measure type   Units_of_Angle

   name                   pole_declination_angle
   version                1.19
   value data type        ASCII_Real
   description            The declination (Dec) of the pole of the specified body, given in angular measurements. 
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   pole_declination_angle_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty of the declination (Dec) of the pole of the specified body, given in angular measurements. 
   unit of measure type   Units_of_Angle

   name                   j2
   version                1.19
   value data type        ASCII_Real
   description            The J2 gravitational harmonic coefficient of the body identified in the enclosing class. 

   name                   j4
   version                1.19
   value data type        ASCII_Real
   description            The J4 gravitational harmonic coefficient of the body identified in the enclosing class. 

   name                   j6
   version                1.19
   value data type        ASCII_Real
   description            The J6 gravitational harmonic coefficient of the body identified in the enclosing class. 

   name                   j8
   version                1.19
   value data type        ASCII_Real
   description            The J8 gravitational harmonic coefficient of the body identified in the enclosing class. 

   name                   gmass
   version                1.19
   value data type        ASCII_Real
   description            The product of the Gravitational constant and the mass of the identified body. 
   unit of measure type   Units_of_Gmass

   name                   grav_ref_radius
   version                1.19
   value data type        ASCII_Real
   description            The reference radius for the gravitational harmonic coefficients of the body identified in the enclosing class. 
   unit of measure type   Units_of_Length

   name                   epoch_ring_fit_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            The epoch for the ring orbital elements given in this product. Format is YYYY-MM-DDTHH:MM:SS.SSSZ and may be truncated. 
   unit of measure type   Units_of_Time

   name                   semimajor_axis
   version                1.19
   value data type        ASCII_Real
   description            The semimajor axis of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Length

   name                   semimajor_axis_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the semimajor axis of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Length

   name                   eccentricity
   version                1.19
   value data type        ASCII_Real
   description            The eccentricity of the orbit of the body or ring identified in the enclosing class. 

   name                   eccentricity_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the eccentricity of the orbit of the body or ring identified in the enclosing class. 

   name                   periapse_longitude
   version                1.19
   value data type        ASCII_Real
   description            The longitude of periapse for the orbit of the body or ring identified in the enclosing class. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   periapse_longitude_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the longitude of periapse for the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angle

   name                   periapse_precession_rate
   version                1.19
   value data type        ASCII_Real
   description            The precession rate of the periapse of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angular_Velocity

   name                   periapse_precession_rate_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the periapse precession rate of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angular_Velocity

   name                   periapse_precession_rate_method
   version                1.19
   value data type        ASCII_Integer
   description            A flag indicating the constraints used to determine the periapse precession rate of the orbit of the body or ring identified in the enclosing class. 

   name                   inclination
   version                1.19
   value data type        ASCII_Real
   description            The inclination of the orbit of the body or ring identified in the enclosing class. 
   minimum value          0
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   inclination_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the inclination of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angle

   name                   node_longitude
   version                1.19
   value data type        ASCII_Real
   description            The longitude of the ascending node of the orbit of the body or ring identified in the enclosing class. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   node_longitude_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the longitude of the ascending node of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angle

   name                   nodal_regression_rate
   version                1.19
   value data type        ASCII_Real
   description            The regression rate of the node of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angular_Velocity

   name                   nodal_regression_rate_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the periapse precession rate of the orbit of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Angular_Velocity

   name                   nodal_regression_rate_method
   version                1.19
   value data type        ASCII_Integer
   description            A flag indicating the constraints used to determine the node regression rate of the orbit of the body or ring identified in the enclosing class. 

   name                   number_points
   version                1.19
   value data type        ASCII_Integer
   description            Number of fitted data points for the orbit of the body or ring identified in the enclosing class. 

   name                   fit_rms_semimajor
   version                1.19
   value data type        ASCII_Real
   description            The RMS residuals for the semimajor axis of the body or ring identified in the enclosing class. 
   unit of measure type   Units_of_Length

   name                   normal_mode_amplitude
   version                1.19
   value data type        ASCII_Real
   description            The amplitude of the normal mode for the ring identified in the enclosing class. A value of -9.99X10^99 indicates there is no normal mode for the ring. 
   unit of measure type   Units_of_Length

   name                   normal_mode_amplitude_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the normal mode of the ring identified in the enclosing class. A value of -9.99X10^99 indicates there is no normal mode for the ring. 
   unit of measure type   Units_of_Length

   name                   normal_mode_phase
   version                1.19
   value data type        ASCII_Real
   description            The phase of the normal mode at epoch specified by epoch_ring_fit_utc for the ring identified in the enclosing class. A value of -9.99X10^99 indicates there is no normal mode for the ring. 
   unit of measure type   Units_of_Angle

   name                   normal_mode_phase_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the value for the normal_mode_phase of the ring identified in the enclosing class. A value of -9.99X10^99 indicates there is no normal mode for the ring. 
   unit of measure type   Units_of_Angle

   name                   normal_mode_pattern_speed
   version                1.19
   value data type        ASCII_Real
   description            The pattern speed of the normal mode in the ring identified in the enclosing class. A value of -9.99X10^99 indicates there is no normal mode for the ring. 
   unit of measure type   Units_of_Angular_Velocity

   name                   normal_mode_pattern_speed_uncert
   version                1.19
   value data type        ASCII_Real
   description            The uncertainty in the pattern speed of the normal mode in the ring identified in the enclosing class. A value of -9.99X10^99 indicates there is no normal mode for the ring. 
   unit of measure type   Units_of_Angular_Velocity

   name                   normal_mode_wavenumber
   version                1.19
   value data type        ASCII_Integer
   description            The wave number of the normal mode in the ring identified in the enclosing class. A value of -999 indicates there is no normal mode for the ring. 

   name                   reprojection_plane
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            reprojection_plane identifies the plane onto which the reprojection is based. Possible values for the Saturn ring system are 'Equator', 'Laplace', 'A', 'B', 'C', 'D', 'E', 'F', 'G', 'Phoebe'. For the Uranus ring system values are 'Equator', 'Laplace', 'Six', 'Five', 'Four', 'Alpha', 'Beta', 'Eta', 'Gamma', 'Delta', 'Lambda','Epsilon',Nu, Mu. Required in labels of ring reprojection products. 

   name                   epoch_reprojection_basis_utc
   version                1.19
   value data type        ASCII_Date_Time_YMD_UTC
   description            The basis epoch for the reprojection used in this product. Format is YYYY-MM-DDTHH:MM:SS.SSSZ and may be truncated. 
   unit of measure type   Units_of_Time

   name                   corotating_flag
   version                1.19
   value data type        ASCII_Short_String_Collapsed
   description            The corotating_flag is a yes-or-no flag that indicates whether or not a corotating frame is used. a table field. 
   minimum characters     1
   maximum characters     1

   name                   corotation_rate
   version                1.19
   value data type        ASCII_Real
   description            The co-rotation rate associated with the data. 
   unit of measure type   Units_of_Angular_Velocity

   name                   corotating_ring_longitude
   version                1.0
   value data type        ASCII_Real
   description            The ring longitude in the rotating frame. The with zero longitude defined at the epoch specified by epoch_reprojection_basis_utc, zero longitude in the corotating frame at time t corresponds to an inertial longitude of (t-epoch)*corotation_rate. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   minimum_corotating_ring_longitude
   version                1.19
   value data type        ASCII_Real
   description            The minimum value in this product for ring longitude in the rotating frame. The with zero longitude defined at the epoch specified by epoch_reprojection_basis_utc, zero longitude in the corotating frame at time t corresponds to an inertial longitude of (t-epoch)*corotation_rate. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

   name                   maximum_corotating_ring_longitude
   version                1.19
   value data type        ASCII_Real
   description            The maximum value in this product for ring longitude in the rotating frame. The with zero longitude defined at the epoch specified by epoch_reprojection_basis_utc, zero longitude in the corotating frame at time t corresponds to an inertial longitude of (t-epoch)*corotation_rate. 
   minimum value          0
   maximum value          360
   unit of measure type   Units_of_Angle

Parsed Input - Classes:

   name                   Body_Ident_Base
   description            The Body_Ident_Base class provides multiple attributes that can be used to identify a physical object (spacecraft, planet instrument, transmitter, system barycenter, etc.). At least one must be used. 
   is abstract            true
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      body_spice_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Frame_Ident_Base
   description            The Frame_Ident_Base class provides multiple attributes that can be used to identify a reference frame. At least one must be used. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      frame_spice_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.comment
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Central_Body_Ident
   description            The Central_Body_Ident class uniquely identifies the body that is the central body associated with an observation (e.g., Saturn for Saturn system observations). 
   is abstract            false
   is choice              false
   subclass of            Body_Ident_Base

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Body_Ident_Base
      minimum occurrences   1
      maximum occurrences   1
      reference type        parent_of

   name                   Reference_Frame_Ident
   description            The Reference_Frame_Ident class is a base class for identifying reference frames. These are frames in the NAIF sense, i.e., three orthogonal axes with a specified orientation, but without a fixed origin. 
   is abstract            false
   is choice              false
   subclass of            Frame_Ident_Base

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Frame_Ident_Base
      minimum occurrences   1
      maximum occurrences   1
      reference type        parent_of

   name                   Display_Direction
   description            The Display_Direction class specifies which two of the dimensions of an Array object should be displayed and how they should be displayed in the vertical (line) and horizontal (sample) dimensions of a display device. This class is a modification of the corresponding class in the Display Dictionary, and is redefined here for convenience. The local_identifier_reference is used to identify the array or arrays to which this iteration of the class applies. Multiple entries are permitted the settings in the iteration of Display_Direction apply to all of the referenced arrays. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.local_identifier_reference
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      pds.comment
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      horizontal_display_axis
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      horizontal_display_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      vertical_display_axis
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      vertical_display_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

   name                   Uniformly_Sampled_Radius
   description             The Uniformly_Sampled_Radius class provides attributes describing the spectral characteristics of an axis of an Array object or the rows of a Table object, in cases where the spectral sampling interval is regular and the sampling parameters are in wavelength units. The axis is identified either by using Local_Internal_Reference, or by using axis name. The latter may be simpler to use if this class applies to multiple Array objects. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      axis_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      sampling_interval_length
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sampling_scale
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sampling_base
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      first_ring_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      last_ring_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.comment
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.Local_Internal_Reference
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

   name                   Occultation_Ring_Profile
   description            This class replaces the Radio_Occultation and Stellar_Occultation classes. It is used for all ring occultation profiles regardless of the occultation type. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      orbit_number
      minimum occurrences   0
      maximum occurrences   unbounded
      reference type        attribute_of

      local identifier      sclk_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sclk_stop_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      occultation_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      occultation_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_profile_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      planetary_occultation_flag
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      data_quality_score
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      data_quality_index
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      ring_detected
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_plane
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      star_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      fresnel_scale
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      projected_star_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sigma_projected_star_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      fractional_error_star_counts
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      time_constant_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      time_constant
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sigma_time_constant
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      dsn_station_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      frequency_band
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      radial_resolution
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      radial_sampling_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_radial_sampling_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_radial_sampling_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      reference_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_event_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_event_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_start_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_stop_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      spacecraft_event_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      spacecraft_event_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_start_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_stop_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      earth_received_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      earth_received_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_radius
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_longitude
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_longitude
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_ring_azimuth
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_ring_azimuth
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sub_stellar_ring_azimuth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sub_stellar_clock_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lowest_detectable_opacity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      highest_detectable_opacity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      along_track_timing_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Occultation_Time_Series
   description            This class supports occultation data organized as a time series.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      orbit_number
      minimum occurrences   0
      maximum occurrences   unbounded
      reference type        attribute_of

      local identifier      sclk_start_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sclk_stop_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      occultation_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      occultation_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      time_series_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      planetary_occultation_flag
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      data_quality_score
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      data_quality_index
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      ring_plane
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      minimum_projected_sun_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_projected_sun_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sigma_projected_sun_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      star_name
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      fresnel_scale
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      projected_star_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sigma_projected_star_diameter
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      fractional_error_star_counts
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      time_constant_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      time_constant
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sigma_time_constant
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      dsn_station_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      frequency_band
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      reference_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_event_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_event_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_start_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_event_stop_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      spacecraft_event_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      spacecraft_event_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_start_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_event_stop_tdb
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      earth_received_start_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      earth_received_stop_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_ring_azimuth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_ring_azimuth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sub_stellar_ring_azimuth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      sub_stellar_clock_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lowest_detectable_opacity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      highest_detectable_opacity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      lowest_detectable_normal_optical_depth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      highest_detectable_normal_optical_depth
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      along_track_timing_offset
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      background_signal
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      average_unocculted_signal
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Occultation_Supplement
   description            This class is required for all radio ring occultation calibration and geometry supplemental files.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      orbit_number
      minimum occurrences   0
      maximum occurrences   unbounded
      reference type        attribute_of

      local identifier      occultation_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      occultation_direction
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_profile_direction
      minimum occurrences   0
      maximum occurrences   2
      reference type        attribute_of

      local identifier      planetary_occultation_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      dsn_station_number
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      frequency_band
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.sampling_parameter_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.sampling_parameter_unit
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.sampling_parameter_interval
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      reference_time_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_event_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_event_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Satellite_Identification
   description            This class identifies the specific satellite to which the parameters given in the enclosing class apply.
   is abstract            false
   is choice              false
   subclass of            Body_Ident_Base

   Associations

      local identifier      Body_Ident_Base
      minimum occurrences   1
      maximum occurrences   1
      reference type        parent_of

   name                   Ring_Identification
   description            This class identifies the specific ring to which the parameters given in the enclosing class apply.
   is abstract            false
   is choice              false
   subclass of            Body_Ident_Base

   Associations

      local identifier      Body_Ident_Base
      minimum occurrences   1
      maximum occurrences   1
      reference type        parent_of

   name                   Normal_Mode_Parameters
   description            This class provides the normal mode parameters is one is present in the described ring.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_amplitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_amplitude_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_phase
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_phase_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_pattern_speed
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_pattern_speed_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      normal_mode_wavenumber
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Global_Model_Parameters
   description            This class provides the general parameters used to generate a ring model.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      epoch_ring_fit_utc
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Reference_Frame_Ident
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

   name                   Central_Body_Parameters
   description            This class provides the parameters used to generate a ring model which are specific to the central body.
   is abstract            false
   is choice              false
   subclass of            Central_Body_Ident

   Associations

      local identifier      gmass
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      grav_ref_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      j2
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      j4
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      j6
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      j8
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pole_right_ascension_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pole_right_ascension_angle_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pole_declination_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pole_declination_angle_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Central_Body_Ident
      minimum occurrences   0
      maximum occurrences   1
      reference type        parent_of

   name                   Satellite_Parameters
   description            This class provides the parameters used to generate a ring model which are specific to a single satellite.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      gmass
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      semimajor_axis
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      semimajor_axis_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      eccentricity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      eccentricity_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      inclination
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      inclination_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Satellite_Identification
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

   name                   Ring_Orbital_Elements
   description            This class provides the orbital element values for a specific ring which were generated in a ring model.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      semimajor_axis
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      semimajor_axis_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      eccentricity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      eccentricity_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      periapse_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      periapse_longitude_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      periapse_precession_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      periapse_precession_rate_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      periapse_precession_rate_method
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      inclination
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      inclination_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      node_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      node_longitude_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      nodal_regression_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      nodal_regression_rate_uncert
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      nodal_regression_rate_method
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      number_points
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      fit_rms_semimajor
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Ring_Identification
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

      local identifier      Normal_Mode_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

   name                   Ring_Model
   description            This class provides the parameters used to generate a ring model.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Global_Model_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Central_Body_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Satellite_Parameters
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

      local identifier      Ring_Orbital_Elements
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

   name                   Reprojection_Geometry
   description            This class provides the parameters describing reprojection geometry when the ring(s) is reprojected based on a fixed grid of coordinates (.g., radius vs. longitude).
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      epoch_reprojection_basis_utc
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      reprojection_plane
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      corotating_flag
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      corotation_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mean_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mean_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_corotating_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_corotating_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Ring_Reprojection
   description            This class provides the parameters used to describe ring reprojection geometry.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Display_Direction
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Central_Body_Parameters
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Ring_Orbital_Elements
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Reprojection_Geometry
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

   name                   Ring_Spectrum
   description            This class provides the parameters used to describe ring spectra or spectrograms.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      pds.local_identifier
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_radius
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      radial_sampling_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_radial_sampling_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_radial_sampling_interval
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_longitude
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_longitude_observed_minus_subsolar
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_longitude_observed_minus_subsolar
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_longitude_observed_minus_subsolar
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      radial_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_radial_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_radial_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      ring_intercept_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_ring_intercept_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_ring_intercept_resolution
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      reflectivity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_reflectivity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_reflectivity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mean_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_observed_ring_elevation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      mean_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_light_source_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      emission_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      minimum_emission_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      maximum_emission_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      Display_Direction
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

   name                   Ring_Moon_Systems
   description            This is an umbrella class for all of the classes and attributes in this dictionary.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      Occultation_Ring_Profile
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Occultation_Time_Series
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Occultation_Supplement
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Ring_Model
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Ring_Reprojection
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

      local identifier      Ring_Spectrum
      minimum occurrences   0
      maximum occurrences   1
      reference type        component_of

End of Report
