PDS4 Local Data Dictionary Processing Report

Configuration:
   LDDTool Version        15.1.0
   LDD Version Id:        1.5.0.0
   LDD Label Version Id:  1.0
   LDD Discipline (T/F):  true
   LDD Namespace URL:     http://pds.nasa.gov/pds4/
   LDD URN Prefix:        urn:nasa:pds:
   Time                   Fri May 24 20:13:15 UTC 2024
   Common Schema          [PDS4_PDS_1M00.xsd]
   Common Schematron      [PDS4_PDS_1M00.sch]
   IM Version Id:         1.22.0.0
   IM Namespace Id:       pds
   IM Label Version Id:   1.0
   IM Object Model        [UpperModel.pont]
   IM Data Dictionary     [dd11179.pins]
   IM Glossary            [Glossary.pins]
   IM Document Spec       [DMDocument.pins]

Parameters:
   Input File             [/home/runner/work/ldd-speclib/ldd-speclib/src/PDS4_SPECLIB_IngestLDD.xml]
   PDS Processing         true
   LDD Processing         true
   Discipline LDD         true
   Mission LDD            false
   Write Attr Elements    false
   Merge with Master      false

Summary:
   Classes                6
   Attributes             78
   Associations           85
   Error messages         0
   Warning messages       0
   Information messages   0

Detailed validation messages

Parsed Input - Header:
   LDD Name               Spectral Library
   LDD Version            1.5.0.0
   Full Name              Susan Slavney
   Steward                geo
   Namespace Id           speclib
   Comment                
        The SPECLIB dictionary contains classes and attributes specific to
        spectral reflectance measurements of laboratory specimens.
        
        SPECLIB version 1.5.0.0 last updated 2023-10-25
        PDS Build 1.18.0.0
        LDDTool version 14.0.13
        Built with lddtool -plJ PDS4_SPECLIB_IngestLDD.xml
    
   Last Modification Time 2023-10-25T17:30Z
   PDS4 Merge Flag        false

Parsed Input - Attributes:

   name                   accumulation_time
   version                1.22
   value data type        ASCII_Real
   description            The duration for which a measurement was acquired. If more than one measurement is reported, this value corresponds to the total measurement time across all measurements.
   minimum value          0
   unit of measure type   Units_of_Time

   name                   ancillary_product_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The ancillary_product_type element provides the type of data found in an ancillary product.
   minimum characters     1
   maximum characters     255

   name                   dark_subtraction_flag
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The dark_subtraction_flag element indicates if a spectrum has been dark subtracted.

   name                   data_producer_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The data_producer_name element provides the name of the creator of the product. For products in RELAB, the value of data_producer_name is always "RELAB".
   minimum characters     1
   maximum characters     255

   name                   data_provider_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The data_provider_name element provides the full name of the person who submitted the product to the library.
   minimum characters     1
   maximum characters     255

   name                   emission_angle
   version                1.22
   value data type        ASCII_Real
   description            The emission_angle element provides the angle between the local vertical at the intercept point and a vector from the intercept point to the sensor.
   nillable               true
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   incidence_angle
   version                1.22
   value data type        ASCII_Real
   description            The incidence_angle element provides the angle between the local vertical at the intercept point and a vector from the intercept point to the source.
   nillable               true
   minimum value          -90
   maximum value          90
   unit of measure type   Units_of_Angle

   name                   instrument_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The instrument_name element provides a descriptive name of the instrument that made a spectral measurement.
   minimum characters     1
   maximum characters     100

   name                   laser_attenuation
   version                1.22
   value data type        ASCII_Real
   description            The laser_attenuation element is the energy of the laser pulse used for sample ablation.
   unit of measure type   Units_of_Energy

   name                   laser_averaged_integrations
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The laser_averaged_integrations element indicates the number of laser integrations that are averaged. A value of 1 means that the integrations are not averaged.

   name                   laser_integrations_saturated
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The laser_integrations_saturated element lists the number of spectra with at least one peak that saturates the spectrometer.

   name                   laser_power_for_calibration_max
   version                1.22
   value data type        ASCII_Real
   description            Maximum laser power, in percent, used during calibration.
   minimum value          0
   maximum value          100

   name                   laser_power_for_calibration_min
   version                1.22
   value data type        ASCII_Real
   description            Minimum laser power, in percent, used during calibration.
   minimum value          0
   maximum value          100

   name                   laser_power_sample
   version                1.22
   value data type        ASCII_Real
   description            Laser power, in percent, utilized during sample analysis.
   minimum value          0
   maximum value          100

   name                   laser_pulses_discarded
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The laser_pulses_discarded element indicates the number of laser pulses discarded.

   name                   laser_pulses_per_integration
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The laser_pulses_per_integration element identifies the number of laser pulses per integration. This value is 1 for single shot spectra.

   name                   laser_pulse_rate
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The laser_pulse_rate element indicates the frequency of laser pulses. A laser_pulse_rate of 10 Hz means that the laser fires ten times per second.
   unit of measure type   Units_of_Frequency

   name                   laser_wavelength
   version                1.22
   value data type        ASCII_Real
   description            Laser wavelength utilized in sample analysis.
   minimum value          0
   unit of measure type   Units_of_Length

   name                   material_common_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The material_common_name element gives the specific name of the specimen material, as specifically as it is known. For example, if a specimen is pure olivine, put "Olivine". If a specimen is a mixture of kaolinite and opal, put "Kaolinite/Opal". Indicate if "Unidentified".
   minimum characters     1
   maximum characters     100

   name                   material_origin
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The material_origin element identifies whether the specimen is natural, synthetic, or natural/doped.
   minimum characters     1
   maximum characters     255

   name                   material_state
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The material_state element identifies the physical state of the specimen.
   minimum characters     1
   maximum characters     255

   name                   material_subtype
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The material_subtype element provides an optional descriptor for additional information about the physical state of the specimen, e.g. particulate or nonparticulate.
   minimum characters     1
   maximum characters     255

   name                   material_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The material_type element indicates the general type of the specimen.
   minimum characters     1
   maximum characters     30

   name                   measurement_atmosphere_composition
   version                1.22
   value data type        UTF8_Text_Preserved
   description            The measurement_atmosphere_composition element identifies any gas(es) present in measurement environment.
   nillable               true
   minimum characters     1
   maximum characters     1000

   name                   measurement_atmosphere_description
   version                1.22
   value data type        UTF8_Text_Preserved
   description            The measurement_atmosphere_description decribes the atmospheric conditions through which the data was taken.
   minimum characters     1
   maximum characters     1000

   name                   measurement_atmosphere_pressure
   version                1.22
   value data type        ASCII_Real
   description            The measurement_atmosphere_pressure element provides the atmospheric pressure of the measurement environment.
   nillable               true
   unit of measure type   Units_of_Pressure

   name                   measurement_atmosphere_relative_humidity
   version                1.22
   value data type        ASCII_Real
   description            The measurement_atmosphere_relative_humidity element provides the relative humidity of the measurement environment.
   nillable               true
   minimum value          0
   maximum value          100

   name                   measurement_atmosphere_temperature
   version                1.22
   value data type        ASCII_Real
   description            The measurement_atmosphere_temperature element provides the temperature of the measurement environment.
   nillable               true
   unit of measure type   Units_of_Temperature

   name                   measurement_date_time
   version                1.22
   value data type        ASCII_Date_Time_YMD
   description            The measurement_date_time element identifies the date and time of the observation and measurement.
   nillable               true

   name                   measurement_geometry_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The measurement_geometry_type element identifies the type of geometry at which a measurement is taken.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   measurement_location_number
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The measurement_location_number element indicates the location number of spectra collection on the target surface.

   name                   measurement_locations_per_sample
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The measurement_locations_per_sample element indicates the number of measurement locations per sample.

   name                   measurement_notes
   version                1.22
   value data type        UTF8_Text_Preserved
   description            The measurement_notes element contains relevant notes about how a measurement was made.
   minimum characters     1
   maximum characters     1000

   name                   measurement_reference_standard
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The measurement_reference_standard element identifies the standard object on which observations are performed in order to calibrate a measurement.
   minimum characters     1
   maximum characters     255

   name                   measurement_requestor
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The measurement_requestor element identifies the individual or laboratory who requested the measurement. The attribute may be present with a null value. A maximum of two names are permitted.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   measurement_run
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The measurement_run element identifies the run number of the measurement in a particular day.
   nillable               true

   name                   measurement_segments
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The measurement_segments are the number of individual spectra that were combined to create the final merged spectrum. If the spectrum is not merged from multiple spectra, then the value of measurement_segments is 1.

   name                   measurement_source_description
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The measurement_source_description element identifies the source used for the measurement such as the type of lamp, heating element, laser, or radioactive source.
   minimum characters     1
   maximum characters     255

   name                   measurement_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The measurement_type element identifies the type of spectroscopy performed on a specimen.
   minimum characters     1

   name                   microscope_objective
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The microscope_objective is the magnification power of the objective lens by power (e.g. 4x, 10x).
   minimum value          0

   name                   mineral_subtype
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The mineral_subtype element identifies the mineral subtype of the specimen.
   minimum characters     1
   maximum characters     255

   name                   mineral_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The mineral_type element identifies the type of mineral to which the specimen belongs.
   minimum characters     1
   maximum characters     255

   name                   organic_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The organic_type element identifies the organic type to which the specimen belongs.
   minimum characters     1
   maximum characters     255

   name                   phase_angle
   version                1.22
   value data type        ASCII_Real
   description            The phase_angle element provides the angle between incidence and emission vectors.
   nillable               true
   minimum value          -180
   maximum value          180
   unit of measure type   Units_of_Angle

   name                   processing_description
   version                1.22
   value data type        UTF8_Text_Preserved
   description            The processing_description element provides information about how measurement(s) for a particular product were made, in addition to the information given in the Measurement Parameters class. In the case of a product created by merging multiple measurements, this element describes how the merge was done.

   name                   rock_subtype
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The rock_subtype element identifies the rock subtype of the specimen.
   minimum characters     1
   maximum characters     255

   name                   rock_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The rock_type element identifies the type of rock the specimen is.
   minimum characters     1
   maximum characters     255

   name                   segment_number
   version                1.22
   value data type        ASCII_NonNegative_Integer
   description            The segment_number element identifies which segment of a merged spectrum is described by a Measurement_Parameters class. The first segment is segment number 1. If the spectrum is not merged from multiple segments, then the value of segment_number is 1.

   name                   source_specimen_id
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The source_specimen_id element identifies the source specimen from which the observed specimen is derived.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   specimen_collection_location
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_collection_location element provides the place where the specimen was collected.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   specimen_owner_location
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_owner_location element provides the institution or laboratory name where the specimen resides.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   specimen_owner_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_owner_name element identifies the individual or laboratory to whom the specimen belongs.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   specimen_description
   version                1.22
   value data type        UTF8_Text_Preserved
   description            The specimen_description element provides a short description of the specimen.
   minimum characters     1
   maximum characters     1000

   name                   specimen_dilution_method
   version                1.22
   value data type        UTF8_Text_Preserved
   description            The specimen_dilution_method element describes the method by which dilution was conducted.
   minimum characters     1
   maximum characters     1000

   name                   specimen_id
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_id element uniquely identifies the specimen.
   minimum characters     1
   maximum characters     255

   name                   specimen_max_size
   version                1.22
   value data type        ASCII_Real
   description            The specimen_max_size element identifies the maximum particle size of the observed specimen.
   minimum value          0
   unit of measure type   Units_of_Length

   name                   specimen_max_size_reported_percentile
   version                1.22
   value data type        ASCII_Real
   description            The percentile reported by the specimen_max_size element. For example, a specimen_max_size_reported_percentile of 90 indicates that 90 percent of the specimen has a particle size less than or equal to specimen_max_size.
   minimum value          0
   maximum value          100

   name                   specimen_min_size
   version                1.22
   value data type        ASCII_Real
   description            The specimen_min_size element identifies the minimum particle size of the observed specimen.
   minimum value          0
   unit of measure type   Units_of_Length

   name                   specimen_min_size_reported_percentile
   version                1.22
   value data type        ASCII_Real
   description            The percentile reported by the specimen_min_size element. For example, a specimen_min_size_reported_percentile of 90 indicates that 90 percent of the specimen has a particle size greater than or equal to specimen_min_size.
   minimum value          0
   maximum value          100

   name                   specimen_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_name element identifies the specimen as it is named where it is being kept.
   minimum characters     1
   maximum characters     255

   name                   specimen_ph
   version                1.22
   value data type        ASCII_Real
   description            The specimen_ph element provides the pH of the observed specimen.
   minimum value          0
   maximum value          14

   name                   specimen_provider_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_provider_name element gives the name of the person who provided the specimen for spectral measurement.
   minimum characters     1
   maximum characters     255

   name                   specimen_solute_standard
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_solute_standard element provides the standard used for the solute.
   minimum characters     1
   maximum characters     255

   name                   specimen_thin_section_flag
   version                1.22
   value data type        ASCII_Short_String_Collapsed
   description            The specimen_thin_section_flag element indicates whether or not the specimen is a thin section.

   name                   specimen_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The specimen_type element gives one or two terms that classify the origin of the specimen. 
   minimum characters     1
   maximum characters     255

   name                   spectral_range_max
   version                1.22
   value data type        ASCII_Real
   description            The spectral_range_max element identifies the maximum value at which a given data item was sampled. For example, a spectrum that was measured in the 0.4 to 3.5 um spectral range would have a spectral_range_max value of 3.5.
   minimum value          0

   name                   spectral_range_min
   version                1.22
   value data type        ASCII_Real
   description            The spectral_range_min element identifies the minimum value at which a given data item was sampled. For example, a spectrum that was measured in the 0.4 to 3.5 um spectral range would have a spectral_range_min value of 0.4.
   minimum value          0

   name                   spectral_range_parameter_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The spectral_range_parameter_name element identifies the name of the parameter which determines the sampling interval of the measurement.
   minimum characters     1
   maximum characters     255

   name                   spectral_range_unit_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The spectral_range_unit_name element identifies the unit of measure for the values specified by spectral_range_min and spectral_range_max.
   minimum characters     1
   maximum characters     255

   name                   spectral_resolution_width_max
   version                1.22
   value data type        ASCII_Real
   description            The spectral_resolution_width_max element identifies the full width at half maximum (FWHM) of a spectral band in a given spectrum. If all bands are the same width, spectral_resolution_width_min and spectral_resolution_width_max will have the same value.
   nillable               true

   name                   spectral_resolution_width_min
   version                1.22
   value data type        ASCII_Real
   description            The spectral_resolution_width_min element identifies the full width at half minimum (FWHM) of a spectral band in a given spectrum. If all bands are the same width, spectral_resolution_width_min and spectral_resolution_width_max will have the same value.
   nillable               true

   name                   spectral_resolution_width_unit_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The spectral_resolution_width_unit_name element identifies the unit of measure for the values specified by spectral_resolution_width_min and spectral_resolution_width_max.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   spectral_sampling_interval_max
   version                1.22
   value data type        ASCII_Real
   description            The spectral_sampling_interval_max element identifies the maximum distance between band centers in a given spectrum. If all band centers are equally spaced, spectral_sampling_interval_min and spectral_sampling_interval_max will have the same value.
   nillable               true

   name                   spectral_sampling_interval_min
   version                1.22
   value data type        ASCII_Real
   description            The spectral_sampling_interval_min element identifies the minimum distance between band centers in a given spectrum. If all band centers are equally spaced, spectral_sampling_interval_min and spectral_sampling_interval_max will have the same value.
   nillable               true

   name                   spectral_sampling_interval_unit_name
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The spectral_sampling_interval_unit_name element identifies the unit of measure for the values specified by spectral_sampling_interval_min and spectral_sampling_interval_max.
   nillable               true
   minimum characters     1
   maximum characters     255

   name                   synthetic_processing_description
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The synthetic_processing_description element describes how a synthetic specimen has been processed.
   minimum characters     1
   maximum characters     255

   name                   synthetic_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The synthetic_type element identifies the process by which the specimen was produced synthetically.
   minimum characters     1
   maximum characters     255

   name                   volatile_type
   version                1.22
   value data type        UTF8_Short_String_Collapsed
   description            The volatile_type element indicates whether the material was volatile-poor (less than 2.0% loss on ignition) or volatile-rich (greater than 2.0% loss on ignition). 
   nillable               true
   minimum characters     1
   maximum characters     255

Parsed Input - Classes:

   name                   Measurement_Instrument
   description            The Measurement_Instrument class contains attributes that identify the instrument that made the measurement. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      speclib:instrument_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.Internal_Reference
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

   name                   Measurement_Parameters
   description            The Measurement_Parameters class contains attributes relevant to a single measurement of a specimen. 
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      speclib:segment_number
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_range_parameter_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_range_min
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_range_max
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_range_unit_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_sampling_interval_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_sampling_interval_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_sampling_interval_unit_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_resolution_width_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_resolution_width_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:spectral_resolution_width_unit_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_run
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_location_number
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_locations_per_sample
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_reference_standard
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_geometry_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:incidence_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:emission_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:phase_angle
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_source_description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_atmosphere_pressure
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_atmosphere_temperature
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_atmosphere_relative_humidity
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_atmosphere_composition
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_atmosphere_description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_date_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:data_producer_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:data_provider_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_requestor
      minimum occurrences   0
      maximum occurrences   2
      reference type        attribute_of

      local identifier      speclib:measurement_notes
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:accumulation_time
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:microscope_objective
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_pulses_per_integration
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_attenuation
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_power_sample
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_power_for_calibration_min
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_power_for_calibration_max
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_wavelength
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_pulse_rate
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_averaged_integrations
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:dark_subtraction_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_pulses_discarded
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:laser_integrations_saturated
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:Measurement_Instrument
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

   name                   Specimen_Classification
   description            The Specimen_Classification class provides information about how a specimen has been classified.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      speclib:specimen_type
      minimum occurrences   1
      maximum occurrences   2
      reference type        attribute_of

      local identifier      speclib:material_common_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:material_origin
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:synthetic_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:material_state
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:organic_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:material_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:material_subtype
      minimum occurrences   0
      maximum occurrences   10
      reference type        attribute_of

      local identifier      speclib:mineral_type
      minimum occurrences   0
      maximum occurrences   *
      reference type        attribute_of

      local identifier      speclib:mineral_subtype
      minimum occurrences   0
      maximum occurrences   10
      reference type        attribute_of

      local identifier      speclib:rock_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:rock_subtype
      minimum occurrences   0
      maximum occurrences   10
      reference type        attribute_of

      local identifier      speclib:volatile_type
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:synthetic_processing_description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_ph
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_dilution_method
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_solute_standard
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Specimen_Parameters
   description            The Specimen_Parameters class provides information about a specimen for which measurements have been made.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      speclib:specimen_id
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:source_specimen_id
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_min_size
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_min_size_reported_percentile
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_max_size
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_max_size_reported_percentile
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_thin_section_flag
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_collection_location
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_owner_location
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_owner_name
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:specimen_provider_name
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

   name                   Ancillary_Product
   description            The Ancillary_Product class identifies an ancillary measurement related to a Spectral Library specimen.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      speclib:ancillary_product_type
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      pds.Internal_Reference
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

   name                   Spectral_Library_Product
   description            The Spectral_Library_Product class provides information about a data product in the Spectral Library.
   is abstract            false
   is choice              false
   subclass of            USER

   Associations

      local identifier      speclib:processing_description
      minimum occurrences   0
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:measurement_segments
      minimum occurrences   1
      maximum occurrences   1
      reference type        attribute_of

      local identifier      speclib:Specimen_Parameters
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

      local identifier      speclib:Specimen_Classification
      minimum occurrences   1
      maximum occurrences   1
      reference type        component_of

      local identifier      speclib:Measurement_Parameters
      minimum occurrences   1
      maximum occurrences   *
      reference type        component_of

      local identifier      speclib:Ancillary_Product
      minimum occurrences   0
      maximum occurrences   *
      reference type        component_of

End of Report
